<EEPROM.h>

EEPROM.begin(EEPROM\_SIZE); // number of bytes to use, 17

EEPROM.write(address, data); // address from 0 to 16

EEPROM.commit();

Int Data = EEPROM.read(address);